# This is a Revit shared parameter file.
# Do not edit manually.
*META	VERSION	MINVERSION
META	2	1
*GROUP	ID	NAME
GROUP	1	OPRAWY OŚWIETLENIOWE
*PARAM	GUID	NAME	DATATYPE	DATACATEGORY	GROUP	VISIBLE	DESCRIPTION	USERMODIFIABLE
PARAM	00936410-834d-4833-b551-2ea54296e507	Number of on/off switcing cycles before premature lamp failure	NUMBER		1	1		1
PARAM	6275c211-c64c-4c2a-a81d-c2c824ba5644	Lamp power factor	NUMBER		1	1		1
PARAM	0c99a413-0abf-44ca-a94a-6c5b167a9d3c	Rated lamp lifespan	TEXT		1	1		1
PARAM	2c26c71b-f81a-43e1-b227-eb1315407cd1	Light source	TEXT		1	1		1
PARAM	de5e421c-57bb-497b-8639-ba54947e0811	Units per package	NUMBER		1	1		1
PARAM	af7ec929-4b5f-4160-8911-1e9fd601cbf4	Warm-up to 60% of total luminous flux	TEXT		1	1		1
PARAM	e055e92b-206b-4943-87fd-c534ef5e29f8	Energy efficiency class	TEXT		1	1		1
PARAM	0317e732-3ca3-4aee-a14c-49a2ac8b2b86	Lumen maintenance	NUMBER		1	1		1
PARAM	41383935-340d-4a81-9816-700384df415b	Impact resistance IK	TEXT		1	1		1
PARAM	f550d639-9146-4b96-bec5-0a3976e734ea	For outdoor use	YESNO		1	1		1
PARAM	bd75ea3f-c310-4027-aace-e3cb38e79b81	Compability with dimmers	TEXT		1	1		1
PARAM	dc0f2044-b680-4edb-b88a-a6f9af6e0b39	Mounting dimensions	TEXT		1	1		1
PARAM	db6dd847-f580-4d1a-b2e3-b2edff2721d3	Dimensions	TEXT		1	1		1
PARAM	dab93b4c-1802-4085-a921-585814eef11b	Nominal lamp lifespan	TEXT		1	1		1
PARAM	60d59e4e-3e9f-4294-b946-936227313563	Version	TEXT		1	1		1
PARAM	fdb0b64e-93ec-49b2-8931-a12c26f5880e	Electrical protection class	TEXT		1	1		1
PARAM	0f878853-d937-45e2-92db-0d4f5e359432	RCR/PIR	TEXT		1	1		1
PARAM	d99d4354-fb3d-4d27-adcd-95605329c695	Rated power	ELECTRICAL_WATTAGE		1	1		1
PARAM	d5bc5d55-25fc-41f4-bb2b-84cdcfc54896	Material of the diffuser	TEXT		1	1		1
PARAM	83378460-eabf-4fad-8c55-fa308126fe4c	Clips	TEXT		1	1		1
PARAM	ce26d96a-e5cc-4d53-a21a-f5d06808fff2	Luminous efficacy	ELECTRICAL_EFFICACY		1	1		1
PARAM	be16df71-0572-4f74-9bbd-dd73afaae63f	Replaceable light source	YESNO		1	1		1
PARAM	88128778-ecfd-4e04-ba26-76c5eb23d112	Net weight of 1 unit	MASS		1	1		1
PARAM	a7c7197b-4688-4871-b75c-c0d3a6d72fca	Spectral power distribution	TEXT		1	1		1
PARAM	c07e4780-8b42-4884-b0c3-accb8cc98a05	Emergency lighting	TEXT		1	1		1
PARAM	32b8d984-a942-4e78-a7f7-6cf7db7cfb2d	Type of the diffuser	TEXT		1	1		1
PARAM	5d2b668a-4180-4d04-9dc2-9af5d9f887e1	Supply voltage	TEXT		1	1		1
PARAM	7e05a88a-63cd-44b4-9d34-37a5350516d1	Ingress protection IP	TEXT		1	1		1
PARAM	37843595-254a-4600-8da0-6663743d9f6c	Color uniformity	TEXT		1	1		1
PARAM	1f3b2e9e-7acc-40fe-aa37-8ef46713a7d1	Colour rendering	TEXT		1	1		1
PARAM	78674eaa-a110-4f09-b929-c0f525811f1f	Failure 5000h	TEXT		1	1		1
PARAM	b18d77b6-9967-426e-9f4a-6878cc28f59b	Index	TEXT		1	1		1
PARAM	08e1bfbb-c05c-4ec3-a9ec-3cbdf7fadee3	Power supply	TEXT		1	1		1
PARAM	2f021ec2-8537-481a-a131-82368ff09680	Packages per collective packing	NUMBER		1	1		1
PARAM	32437cc7-7582-4b63-a031-9b066277bb62	Nominal radiation angle	ANGLE		1	1		1
PARAM	8a4cacc8-eac4-4081-8c7d-e5fd9c754521	Colour temperature	COLOR_TEMPERATURE		1	1		1
PARAM	d54005cd-aa24-46fa-89b8-aae545e7b3aa	Frequency	TEXT		1	1		1
PARAM	1fb7afd1-2d84-40a8-a26b-2fbba51e48f7	Rated power luminaire	ELECTRICAL_WATTAGE		1	1		1
PARAM	abcbb9d9-76ea-43cb-868d-6a88eb1da489	Material of body	TEXT		1	1		1
PARAM	bc09c2f2-0bba-4944-b130-4edb7e154535	Luminous flux	ELECTRICAL_LUMINOUS_FLUX		1	1		1
PARAM	d03c59f5-171f-4f9d-9295-264e66cfcbe4	(EAN) European Article Number	TEXT		1	1		1
